Specification Sheet	Page:	1
 No.:	1	QTY:	2	 Product no.:
 Tag no.	VAA,VAB
 Service	<Option>
	  SV0703-102    Indicating unit : "bar"
< Specification >
   Model	AGVM
   Description	 Top-Guided Single-Seat Control Valves	  SV0601-001    Air piping Connection: 1/4 NPT
   Valve size	1-1/2	inch	  SV0018-005    Oil-free Gr.B (For stainless steel 
	   Port size	1	inch	body)  and Water-free treatment
   Rated Cv	14
   Connection size	inch	      
   Body rating	ANSI300
   End connection	BW	      
   Body material	A351CF8
   Trim material	SUS316 STELLITE
   Flow characteristic	EQ%	      
   Bonnet type	EXTENTION-2
   Actuator	PSA1	      
   Manual operator	---
   Valve action	REVERSE(Air fail close)
   Gland packing	V-PTFE	      
   Gasket	V7590/V563(PTFE)
   Grease
	      
   Air supply	2.7bar
   Spring range	0.8-2.4bar
< Accesories >	      
   Positioner / Signal	HTP-1D
       Exprosion-proof	FM Explosionproof and Flameproof, 1/4 NPT, 	      
       Signal	0.2-1.0 bar
   Regurator	KZ03-2B-XX
   Regulator 2	      
   Limit Switch
        Action	      
   Solenoid valve
        Action
        Power supply	<Finish>
   Others	     Body:	M10B5/10
 	     Diaph. Case:	M10B5/10
 	     Yoke:	M10B5/10
	     Paint:	Standard
<Operating condition>	<Seat Leakage>
   Fluid name	Liquid Nitrogen	[	LIQUID	]	CLASS IV (SV0201-003)
	 	MAX	NOR	MIN	UNIT
   Flow rate	770	770	l/h	<Note>	Tokumi	-
   Inlet pressure	11	11	barG
   Outlet pressure	10.8	10.8	barG
   Diff. pressure	0.2	0.2	bar
   Shut-off press.	25	bar
   Temperature	-196	-196	degC
   Sp.Gr. (liq.)	1.2507	1.2507	water=1
   	MW
   Viscosity	cP
   Flash	%	<Line spec>
   Velocity	0.18	0.18	m/s	Design press.	25	barG
   S.P.L.	40	40	dBA	Design temp.	-196	degC
   Calculated Cv	2.226	2.226	 	Line size  in/out	1-1/2	1-1/2	inch
   Travel	50	50	%	Line Sch. / Thick.	40S	mm
463: Cryolor/ Low Temp     Rev.1	YAMATAKE

	 Specification Sheet	Page:	2
 No.:	2	QTY:	1	 Product no.:
 Tag no.	VB
 Service	<Option>
	  SV0703-102    Indicating unit : "bar"
< Specification >
   Model	AGVM
   Description	 Top-Guided Single-Seat Control Valves	  SV0601-001    Air piping Connection: 1/4 NPT
   Valve size	1	inch	  SV0018-005    Oil-free Gr.B (For stainless steel 
	   Port size	Cv=0.63	inch	body)  and Water-free treatment
   Rated Cv	0.63
   Connection size	inch	      
   Body rating	ANSI300
   End connection	BW	      
   Body material	A351CF8
   Trim material	SUS316 STELLITE
   Flow characteristic	EQ%	      
   Bonnet type	EXTENTION-2
   Actuator	PSA1	      
   Manual operator	---
   Valve action	REVERSE(Air fail close)
   Gland packing	V-PTFE	      
   Gasket	V7590/V563(PTFE)
   Grease
	      
   Air supply	2.7bar
   Spring range	0.8-2.4bar
< Accesories >	      
   Positioner / Signal	HTP-1D
       Exprosion-proof	FM Explosionproof and Flameproof, 1/4 NPT, 	      
       Signal	0.2-1.0 bar
   Regurator	KZ03-2B-XX
   Regulator 2	      
   Limit Switch
        Action	      
   Solenoid valve
        Action
        Power supply	<Finish>
   Others	     Body:	M10B5/10
 	     Diaph. Case:	M10B5/10
 	     Yoke:	M10B5/10
	     Paint:	Standard
<Operating condition>	<Seat Leakage>
   Fluid name	Liquid Nitrogen	[	GAS	]	CLASS IV (SV0201-003)
	 	MAX	NOR	MIN	UNIT
   Flow rate	5	m3/h[N]	<Note>	Tokumi	-
   Inlet pressure	14	barG
   Outlet pressure	13.8	barG
   Diff. pressure	0.2	bar
   Shut-off press.	25	bar
   Temperature	-40	degC
   Sp.Gr. (liq.)	water=1
   	28.02	MW
   Viscosity	cP
   Flash	%	<Line spec>
   Velocity	0	Mach	Design press.	25	barG
   S.P.L.	40	dBA	Design temp.	-196	degC
   Calculated Cv	0.1109	 	Line size  in/out	3	3	inch
   Travel	53	%	Line Sch. / Thick.	40S	5.5	mm
463: Cryolor/ Low Temp     Rev.1	YAMATAKE