12. Monitoring
A monitoring screen is composed of
2 screens.
The monitoring screen (page 1)
shows output, input, LRV (0%),
URV (100%), and input angle.
Tapping [Start periodic updates]
starts automatic periodic updating of
input value.
Tapping [Stop periodic updates]
stops automatic periodic updating of
input value.
Tap [Next>] to show page 2 of the
monitoring.
Page 2 of the monitoring screen
shows input angle, angle at 0%,
angle at 100%, offset angle, torque
tube temperature, and angle sensor
temperature.
Tapping [Start periodic updates]
starts automatic periodic updating of
input value.
Tapping [Stop periodic updates]
stops automatic periodic updating
of input value.
Tap [<Prev.] to show page 1 of the
monitoring.