11. Input Range
Sets the input signal range.
LRV is the input signal value that closes
the valve fully. URV is the input signal
value that opens the valve 100%.
Tap any display field to display the input
screen. Input the value and tap [Enter].
Tap [Send] to transmit the changes to
the valve positioner. If you have not yet
tapped [Send], and want to recall the
previous data, tap [Read].
To read the current input values, tap
[Read Input Signal].