5. All Functions
Displays all functions.
Additional functions available with the
device software version or device mode
noted:
-- 4-20 mA Correct (valid only for
analog mode)
-- PP Range (valid if DE multi-PV mode
are selected, and PV2 output is on.)
-- PT Range (valid if DE multi-PV mode
are selected, and PV3 output is on,
except the measured gas is
saturated steam.)
-- Measured Gas (ver. 7.8 and later)
-- DE Output Mode (DE mode and
multi-PV)