15. Adjustment
Select the sensor to be adjusted.
-- DP Adjustment: Adjustment of the
differential pressure sensor
-- PP Adjustment: Adjustment of the
static pressure sensor
-- PT Adjustment: Adjustment of the
process temperature sensor
After selection of a sensor, the output
will automatically change to the output
of the sensor being adjusted.
The ranges for the PP (static pressure)
and PT (process temperature) analog
outputs may also be set.
PT Adjustment is not valid if the
measured gas is saturated steam.