1. Summary
A summary screen is composed of 2
screens.
The summary screen (page 1) shows
output, input, LRV (0%), URV (
100%), float length, and specific
gravity (the specific gravity
difference).
Tap [Read output and input] to
update the values. Tap [Next>] to
show page 2 of the summary.
Page 2 of the summary screen
shows input angle, angle at 0%,
angle at 100%, offset angle, torque
tube temperature, and angle sensor
temperature.
Tap [Read input and temp.] to
update the values. Tap [<Prev.] to
show page 1 of the summary.