8. Range
<MagneW 2W>
Sets the flow rate range.
The flow rate range (i.e., max. for
range), flow rate unit, and low-flow
range), flow rate unit,specific gravity
and low-flow cutoff are
configurable.
The maximum flow rate setting is
12 m/s.
The gravity is not shown unless a
mass flow rate unit is selected as the
flow rate unit.
<MagneW 4W>
Sets the flow rate range.
The flow rate range (i.e., max. for
range), flow rate unit,specific gravity
and low-flow cutoff are configurable.
The maximum flow rate setting is
12 m/s.
The range 2 may not be shown
unless the dual range or the normal/
reverse range is selected.
The gravity is not shown unless a
mass flow rate unit is selected as the
flow rate unit.