17. Dummy Input Signal
Enter simulated input signals from
CommPad to control the valve instead of
input signals from the controller.
Tap [0%], [25%], [50%], [75%], or
[100%] to move the valve to the
respective travel position. Tapping
[Clear] will allow input signals from the
controller to control the valve travel.
To read the current travel value and
drive signal (where the control output is
the value of the current to the coil), tap
[Read].
To set an arbitrary value, tap [Set any value].