23. PP Range
Sets range of PP sensor (static
pressure sensor).
Note: Settings for PP Range are only
valid if DE mode and multi-PV are
selected. In other cases, set range
on PP Adjustment screen.
-- PP LRV: Lower value of static
pressure range. Enter value
corresponding to 0% output.
-- PP URV: Upper value of static
pressure range. Enter value
corresponding to 100% output.
-- PP Span: Static pressure output
span, = |URV - LRV|
-- PP URL: Upper limit of the static
pressure output range (the
highest settable value)