19. Remote-seal
Configures the parameters for a
remote sealed transmitter.
-- Auto Range (closed tank):
Automatically calculates the range
(LRV and URV). The user must
enter the high pressure flange
location, specific gravity, fill fluid,
span, flange span, and distance of
the zero level above the lower
flange. This function is valid when
conformity is linear.
-- Set LRV (Actual): When the tank
liquid level is known, this function
is used to shift the range (LRV-
URV) so that the current output
level becomes the percentage of
output specified by the user. This
function is valid when conformity
is linear.
-- Ambient Temperature
Compensation: Compensates for
the effects of temperature on the
fill fluid. The user must enter the
flange span or fill fluid type.