16. Calibration
Select the sensor to be calibrated.
-- DP Calibration: Calibration of the
differential pressure sensor
-- PP Calibration: Calibration of the
static pressure sensor
-- PT Calibration: Calibration of the
process temperature sensor
After selection of a sensor, the output
will automatically change to the output
of the sensor being adjusted.
PT Calibration is not valid if the
measured gas is saturated steam.