12. Calibration
Calibrates the device. There are five
functions.
For a remote-seal transmitter, calibrate
with the height set to 0 meters.
-- Correct zero input: Calibrates zero
input by equalizing input pressures
of HP and LP.
-- Correct LRV: Calibrates zero point
(LRV).
-- Correct URV: Calibrates span (URV).
-- Restore factory settings: Return to
the factory default calibration data.
-- Reset corrections: Discards
calibrations.