10. Dummy Input
Calculates the expected output by
entering dummy inputs.
When the inputs are replaced by
dummy inputs, the color of the
letters changes to orange, and the
names change to dummy DP, dummy
PP, and dummy PT.
-- Comp. Coef.: The compensation
coefficient
-- Output: The simulated output
-- Ref. PT: The reference process
temperature
-- Ref. PP: The reference static
pressure
-- PP ELV.: The elevation (altitude)
of the static pressure
Temperature input is not valid if the
measured gas is saturated steam.
[Output Calc.] is not available if
conformity is square root (flow) and
flow mode is bi-direction.