18. Dummy Drive Signal
Enter simulated drive signals from
CommPad to control the valve instead of
input signals from the controller.
Tap [0%], [25%], [50%], [75%], or
[100%] to move the valve to the
respective travel position for the drive
signal. Tapping [Clear] will allow the
input signals from the controller to
control the valve travel.
To read the current travel value, tap
[Read].
To set an arbitrary value, tap [Set any
value].