25. Records
Past calibration values and a history
of the diagnostics are displayed.
There are three functions.
-- Zero Calibr. Log in CommPad:
Displays the difference between
the zero point (LRV) value, and its
value when the product was
shipped from the factory. The
data at the time the command
was executed by CommPad will
be saved.
-- Zero Calibr. Log in Device:
Displays the difference between
the internal zero point (LRV)
value, and its value when the
product was shipped from the
factory.
-- Status Records: History of status
is displayed.