1. Summary
The summary screen (page 1) shows
output, DP Input, PP Input, PT Input,
and conformity. PT Input is not valid if
the measured gas is saturated steam.
Tap [Read output and input] to update
the values. Tap [Next>] to show page
2 of the summary.
Page 2 of the summary screen shows
PV1-PV3 and SV1-SV3.
PV3 and SV3 are not valid if the
measured gas is saturated steam.
If PV2-PV3 or SV1-SV3 are off, a
hyphen replaces the numerical value.