16. 4-20 mA Correct
Calibration of the 4 mA and 20 mA
output by connecting device to an
accurate meter.
-- Correct 4 mA: Tapping this button
will put device into constant 4 mA
output mode. Tap [Up] or [Down] so
that the meter reading is as close to
4 mA as possible.
-- Correct 20 mA: Tapping this button
will put device into constant 20 mA
output mode. Tap [Up] or [Down] so
that the meter reading is as close to
20 mA as possible.