24. PT Range
Sets range of PT sensor (process
temperature sensor).
Note: Settings for PT Range are only
valid if DE mode and multi-PV are
selected. In other cases, set range
on PT Adjustment screen.
-- PT LRV: Lower value of process
temperature range. Enter value
corresponding to 0% output.
-- PT URV: Upper value of process
temperature range. Enter value
corresponding to 100% output.
-- PT Span: Process temperature
output span, = |URV - LRV|
-- PT URL: Upper limit of the
process temperature output range
(the highest settable value)
-- PT LRL: Lower limit of the
process temperature output range
(the lowest settable value)