10. Control Configuration
Sets the actuator size and gland packing
type parameters.
Select the desired setting from the
combo boxes. If you have not yet tapped
[Send], and want to recall the previous
data, tap [Read].
These parameters are set automatically
by Auto Setup.
The positioner's PID parameters can be
manually set by selecting Param 0 for
the actuator size. (Param selections
range from 0 to 9, and from A to C.)