6. Tag
Displays and writes Tag No.
Tap the tag to modify its value. Tap the
enter key to confirm the value, and then
tap [Send] to transmit the data to the
valve positioner. If you have not yet
tapped [Send], and want to recall the
previous tag, tap [Read].
Up to eight characters may be entered.
Valid characters are A-Z, 0-9, space,
period, hyphen, and slash. Lowercase a-
z will be capitalized to A-Z.