24. Alarm/Contact Output
Sets the alarm/contact output.
There are two types of alarm, output
and sensor temperature.
When an alarm is detected, a record of
it is saved in the device history log, and
the indicator alerts the user to the
occurrence of an alarm.
You can select whether or not there is
output to the output contacts when an
alarm is detected.
Two settings allow a choice of whether
the contact output circuit is open or
closed when an alarm is detected.