9. Pulse
<MagneW 2W>
Sets parameters for pulse output,
namely pulse weight, pulse duty/
pulse width and dropout.
The pulse frequency is calculated
and displayed automatically based
on the flow rate range and pulse
weight settings.
The pulse weight setting should be
such that the pulse frequency is
between 0.0001 and 200 Hz.
For the pulse duty, duty 50% and
numerical are selectable. If duty
50% is selected, pulse ON time is
automatically calculated. With the
numerical, the pulse width can be
set freely.
If duty 50% is selected and the
cycle time of the pulse is two
seconds or longer, the pulse ON
time is fixed as one second.
When the numerical is selected, the
pulse width input is available.
<MagneW 4W>
Sets parameters for pulse output,
namely pulse weight, pulse duty/
pulse width and dropout.
The pulse frequency is calculated
and displayed automatically based
on the flow rate range and the
pulse weight settings.
The pulse frequency 2 may not be
shown, depending on the ranging
setting in the opt. functions menu.
The pulse weight setting should be
such that the pulse frequency is
between 0.00006 and 3000 Hz.
For the pulse duty, duty 50% and
the numerical are selectable.
With the duty 50% setting, pulse ON
time is automatically calculated.
With the numerical, the pulse width
can be set freely.
When the duty 50% is selected and
the cycle time of the pulse is two
seconds or longer, the pulse ON time
is fixed as one second.
When the numerical is selected, the
pulse width input is available.