HART AVP DTM
Version 1.0.0.330

Copyright (C) 2010 Yamatake Corporation All Rights Reserved


1 Introduction
===========================
HART AVP DTM is a HART device DTM for the Yamatake SVP HART field device.
Supported FDT version is 1.2.0 and has certification from FDT-JIG for OS below.
* Windows XP Servoce Pack 3
* Windows Vista Service Pack 2


2 Fixed Bugs 
===========================
This is initial release.


3 New Features
===========================
This is initial release.


4 Known Issues
===========================
Some parameters on "online parameter" display does not provide intellisense help description. (ID#90)

Data value display within "In/Out Characteristics" display cannot work correctly if value edit continues while its input rule is broken. (ID#94)

Some parameters cause moving input focus to navigation area when finishing to edit value in its input port. (ID#95)

As for "Auto Setup" procedure within "Basic Setup" display, user cannot recognize the result of the procedure (i.e. success or failure). (ID#99)

Short cut key functionality cannot work while the input focus resides in AVP DTM display. (ID#157)

While processing procedures invoked by buttons in display, "Print" funtion cannot work correctly and shows the empty display. (ID#162)

The value of Polling Addres within "Device Information" and "Review" menu display is fixed to zero. (ID#169)


5 Notes
===========================
* Do not redistribute this software.

