SCHMIDT® Flow Switch SS 20.200

SCHMIDT Technology has explanded their programme of thermal air flow sensors with thermal flow switches. A very compact housing and a very precise switch point identify these new products. Remarkably is also that these sensors can be used at extremely low flow velocities starting from 0,1 m/s and in air polluted by aggressive particles. An optional available sensor coating protects the sensor tip against solvents, acids and leaching. The smoth surface makes the sensor tip easy cleanable and unsusceptible against dust and dirt. Two LEDs indicate the correct operation and the activation of the switching output. The sensor tube is available in different length and thus can be placed at the correct position regardless of the size of the duct.  Applications: Exhaust-air monitoring, cooling air monitoring, flow monitoring in semiconductor machinery, filter monitoring, laboratory exhaust-air control. Technical data: design: immersion sensor with attached transformer. application: free air and guided air in ducts from 65 to 1.000 mm, measuring range 0,06 … 20 m/s, pressure: atmospheric or up to 10 bar. Mounting: Thread M18x1 optional flange or through passage. Power supply: 24 VDC / approx. 100 mA, output: open-collector, display: 2 LEDs.

SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen,Tel.:  +49/7724/899-0, Fax:+49/7724/899101, Email: info@schmidttechnology.de, Homepage: www.schmidttechnology.de