SCHMIDT® Flow Sensor Family SS 30.300

SCHMIDT Technology presents a completely new family of Inline flow sensors. This is a significant improvement of the SCHMIDT programme of flow sensors which previously consisted of immersion type flow sensors. Inline flow sensor means, that these sensors come with their own measuring pipe thus giving direct display of the volume flow. Contrary to immersion sensors the inline sensors simplify the mounting, reduce the influence of mounting tolerances and the measuring pipe is part of the adjustment process. This new product family consists of 4 sensor models in pipe sizes of ½, 1, 1 ½ and 2 inch. Actual volume flow, totalized volume flow and media temperature can be interrogated from the internal LED display. Two keys allow to configure the functions of the sensor. Output 1 may be configured as switching output or analog output, output 2 may be used as pulse output or second switching output. The new sensors are available from February February 2007.

Applications:
compressed-air consumption measurements, volume flow measurements in test benches, flow measurements in nitrogen or other passivation gases, flow measurements in process gases.

Technical data:
Design:	Inline sensor with integrated electronic and display
Display:	LED 7 segment, red, 4 digits, 7 mm
Pipe sizes:	DN 15 / 25 / 40 / 50  ( ½ , 1, 1 ½, 2 inch)
Measuring range:	75 / 225 / 410 / 700 normal m3/h
Pressure:	up to 16 bar o.p. (230 psig)
Process connection:	Thread R ½, R 1, R 1 ½ , R 2 
Output 1:	switching output or 4 .. 20 mA (user selectable)
Output 2:	Switching output or pulse output (user selectable)
Power supply:	19 … 30 VDC / approx. 100 mA

Manufacturer:
SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen, Phone.:  +49/7724/899-0, Fax:+49/7724/899101, Email: info@schmidttechnology.de, Homepage: www.schmidttechnology.de