SCHMIDT® Strömungs-Sensor SS 20.260

Unter der Bezeichnung SS 20.260 bietet SCHMIDT Technology einen neuen Strömungssensor für Luft und Gase, der sich durch seine sehr kompakte Bauform sowie durch eine robuste Ausführung auszeichnet. Mit einem Messbereich von 20 m/s und seinem linearen Ausgangssignal bietet er sich als universeller Sensor zur Messung von Strömungsgeschwindigkeit, Volumenstrom oder Massenstrom an. Das Sensorelement ist durch den schlagfesten Kammerkopf gegen mechanische Beanspruchung bestens gesichert. Das Fühlerrohr aus Edelstahl ist in verschiedenen Längen zu bekommen, so dass der Sensor sowohl bei kleinen als auch großen Rohren immer in die aerodynamisch beste Position gebracht werden kann. Über zwei Status-LEDs signalisiert der Sensor, ob die Versorgungsspannung ausreicht und ob der Sensor fehlerfrei funktioniert.

Anwendungsbeispiele:
Strömungsmessung in Lüftungskanälen, Durchflussmessung in Prüfständen, Regelung der Verbrennungsluft in Öl-, Kohle-, Holz- oder Gasbrennern, Strömungsregelung in Kühl- und Trocknungsanlagen.

Produktvorteile:
Sehr kompakte Bauform
Einfache Montage
Sehr geringe Stromaufnahme
Fühler vollkommen dicht (IP67)

Technische Daten:
Bauform:	Eintauchsonde mit angebautem Messumformer.
Einsatzbereich:	Frei strömende Luft und geführte Luft in Rohren von 25 bis 500 mm
Medien:	Luft, Stickstoff, Argon und weitere nicht brennbare Gase
Messbereich:	0,2 … 20 m/s
Druck:	atmosphärisch
Montage:	Schraubgewinde
Versorgung: 	24 VDC / Stromaufnahme nur 30 mA
Ausgang: 	0 … 5 V / 0 … 10 V / 4 ... 20 mA linear
Anzeige:	2 Status-LEDs 

SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen,Tel.:  +49/7724/899177, Fax:+49/7724/899101, 
Email: sensors@schmidttechnology.de, Homepage: www.schmidttechnology.de

SCHMIDT® Flow Sensor  SS 20.260

Under the name SS 20.260 SCHMIDT Technology offers a new flow sensor for air and gases which is robust and very compact. It´s measuring range of 20 m/s and linear analog output identify him as universal sensor for measurements of air velocity, volume flow and mass flow in a lot of applications. The sensor is robust due to a chamber in which the sensing element is protected against impacts. The stainless steel sensor tube is available in different length and thus can be placed at the correct position regardless of the size of the duct. Two LED’s indicate the correct operation or inform about wrong supply voltage or sensor defects.

Applications:
Flow measuring in air ducts, volume flow measuring in test benches, control of combustion air of oil, wood, gas or coal burners, flow control in cooling or drying constructions.

Product advantages:
Very compact design
Simple mounting
Low power consumption
Sensor tip completely tight (IP67)

Technical data:
Design:	Immersion sensor with attached transformer
Application:	Free air and guided air in ducts from 25 to 1.000 mm
		(1 to 40 inch)
Medium:	Air, Nitrogen, Argon and other non burnable gases
Measuring range:	0,2 … 20 m/s ( 0.66 … 66 ft/s)
Pressure:	Atmospheric
Mounting:	Thread
Power supply:	24 VDC / power consumption only 30 mA
Output:	0 … 5 V / 0 … 10 V / 4 … 20 mA linear
Display:	2 Status LED’s

Manufacturer:
SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen, Phone.:  +49/7724/899-0, Fax:+49/7724/899101, Email: sensors@schmidttechnology.de, Homepage: www.schmidttechnology.de