SCHMIDT® Flow Sensor now also for use in oxygen

Product material, production process and packaging of a special version of the SS 20.60 series has been designed to meet IEC/TR 60877:1999 standard for usage with bio atomic oxygen (O2) containing more than 21%. Sensor tube and tube through passage are of stainless steel 1.4571. The insertion sensor is available in 4 tube lengths from 120 to 400 mm and various electrical interfaces such as voltage, current, impulse, switching, Profibus DB, DeviceNet. Measuring ranges go from 2.5 m/s up to 200 m/s. Each O2 sensors is individually packed and comes with a special instruction for the sensor handling.
SCHMIDT Technology GmbH, Feldbergstr. 1, D-78112 St. Georgen, Tel.+49/7724/8990, Email.: info@schmidttechnology.de, Homepage. www.schmidttechnology.de