SCHMIDT® Flow-Sensor SS 20.60 HT, for high temperature up to 350 °C

SCHMIDT Technology has developed a high temperature version of the SS 20.60 for the application in operating temperature up to 350 °C - for short time even 400 °C.
The sensor differs formally in the white ceramic tip. Most of the modifications have been made inside the sensor and the modules are designed according to the elevated specification.
A complete new designed electronic unit processes the results of measurement and provides a digital and analogue output of flow velocity as well as temperature. The new status indicator displays information about the current flow velocity and the sensors status. Due to the modular concept the unit can also be supplied with field bus interfaces. The sensors with field bus interfaces can calculate Kg/h or m³/min. and thus disburdens the supervising PLC. Additionally the sensor gives access to its status information and allows the PLC to inform the user about defects of the sensor.
Applications:
Mass flow-control of combustion processes, burner control, flow measurement of process gases, volume flow measurement of test stands, Measurement of flow velocity in drying plants and sterilizing processes.

Technical data
Design:		Immersion sensor with integrated transducer
Application:		Free air and guided air in ducts from 25 to 1,000 mm
Measuring range:	0.2 … 20 m/s 
Pressure		atmospheric
Temperature		0 ... 350 °C 
Mounting:		G ½ thread
Analogue output:	0...10 V, 0/4 ... 20 mA
Digital output		Impulse or switching (10 to 100 Hz)
Power supply:		24 V DC / approx. 150 mA 
Field bus version:	Profibus DP, Device Net.

SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen, Tel.: +49 (0) 7724/899-0, Fax:+49 (0) 7724/899-101, e-Mail:, Homepage: www.schmidttechnology.de