SCHMIDT® Flow Sensor for high gas velocity up to 200 m/s

SCHMIDT Technology GmbH offers a smart and rugged family of gas flow sensors they are able to measure up to 200 m/s. So a lot of industry applications are covered for example consumption and leakage measurement in pressured air systems or the air-mass flow in burner and motors. This flow sensor offers a very wide measuring range dynamic of 1:800 – very low flow rate down to 0.2 m/s can be detected as well. Due to the thermal measuring principle there is no need to detect the pressure or temperature to get a very accurate reading. The maximum pressure in the tube is up to 16 bar and the sensor can be used in pipes prom DN 25 up to DN 800. Each sensor with an analog output, in addition, is equipped with a digital output enabling a direct consumption measurement of the air flow by means of a supply meter. In addition the SS 20.60 is available with bus interface for connecting different field buses. The mounting of the sensor is very easy and cost-saving by a tube throughpassage which is multi-removable. At the back of the housing four multi-coulored Led´s indicate the measure measuring range, which is subdivided in four parts (20%, 50%, 80% and 100%). If the measuring range exceeds or a mistake occurs it is shown by changing the Led´s colour. These features give the user the complete information about the sensor function at a glance. 

SCMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen, Tel.: +49/7724/899-0 Fax: +49/7724/899101, Email: info@schmidttechnology.de, Homepage: www.schmidttechnology.de