Programmierkit für SCHMIDT® Strömungs-Sensoren

Mit Hilfe des Programmierkits können die elektrischen Schnittstellen Strom (0 ... 20mA oder 4 ... mA), Spannung (0 ... 2V, 0 ... 5V, 0 ... 10V) sowie die Ansprechzeit, bzw. Dämpfung (0,01 ... 10s) der SCHMIDT® Strömungs-Sensoren SS 20.400 und SS20.415 an die Einsatzanforderungen angepasst werden. Die Schwellwerte der Schaltausgänge OC1 und OC2 sind einstellbar zwischen 0 ... 100% vom Messbereich und die Schaltpolarität ist umkehrbar. Über die Diagnosefunktion können alle Parameter ausgelesen und die Ursache für eventuelle Störungen bestimmt werden. Zum Lieferumfang gehören die Programmierbox, das RS232-Schnittstellenkabel und die bedienerfreundliche Software passend für PC’s mit Windows 2000 oder XP und RS232 Schnittstelle oder optional ein USB-Anschluss Die Programmierbox verfügt über Anzeige-LEDs für die Schaltzustände OC1 und OC2 und dem Strömungssignal-Ausgang. Sie kann entweder über die mitgelieferte 9V Blockbatterie oder über ein externes Steckernetzteil mit 3,5mm Monoklinkenstecker versorgt werden.

SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen, Germany, 
Tel.:  +49/7724/899-0 Fax:+49/7724/899101, Email: info@schmidttechnology.de,
Homepage: www.schmidttechnology.de

Programming Kit for SCHMIDT® Flow Sensors

This programming kit allows the analogue current outputs (0 … 20 mA or 4 … 20 mA), analogue voltage outputs (0 … 2V, 0 … 5V, 0 … 10V) and the response times (0,01 … 10s) of the SCHMIDT® Flow Sensors SS 20.400 and SS 20.415 to be adapted to the operation requirements. Trigger-levels of the switching outputs OC1 and OC2 are adjustable between 0 … 100% of the end value. The polarity can be inverted. The diagnostic function enables to read the sensor parameters and to find the cause of an eventual malfunction. The programming interface includes the programming box, the RS232 interface cable and the user-friendly software suitable for PC's with Windows 2000 or XP with RS232 or optionally USB interface. The programming box is equipped with a luminous diode based display area for the status of OC1, OC2 and the flow signal output of the connected sensor. Power supply is an integrated 9V battery or alternatively via a 3.5 mm mono jack socket an external wall power supply unit.

SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen, Germany,
Tel.:  +49/7724/899-0 Fax:+49/7724/899101, Email: info@schmidttechnology.de, 
Homepage: www.schmidttechnology.de