SCHMIDT® Strömungs-Sensor SS 23.400 ATEX3 

Fa. SCHMIDT Technology erweitert sein Produktprogramm und bietet einen neuen thermischen Strömungssensor für den Einsatz in explosionsgefährdeten Bereichen. Für den Betrieb gemäß ATEX-Richtlinie entwickelt, entspricht der Sensor SS 23.400 der Gerätekategorie 3G und kann somit in der ATEX-Zone 2 eingesetzt werden.
Die Eintauchsonde mit dem 9 mm dünnen Edelstahl-Fühlerror dient der Messung von Strömungsgeschwindigkeit und –richtung von sauber Luft und Gasen. Die Elektronik auf Mikroprozessorbasis ist im Fühlerrohr integriert. Der robuste Sensorkopf schließt bündig daran an und das äußerst schnelle Messelement ist in der aerodynamisch geformten Strömungskammer vor mechanischer Belastung geschützt untergebracht 
Die Messwertausgabe erfolgt über einen Analogausgang mit Strom- oder Spannungssignal, zwei Schaltausgänge signalisieren Strömungsrichtung und Schwellwertüberschreitung.
Über eine serielle Schnittstelle können, mit Hilfe eines Programmierkits, Ansprechzeit, Schwellwert und Schaltpolarität an die Einsatzanforderungen vor Ort angepasst werden.
Anwendungsbeispiele: Lackieranlagen, Strömungsmessung von Gasen, Überwachung von Abzugshauben, Durchflussmessung in medizinischen Geräten und Prüfständen
Technische Daten: Gerätekennzeichnung: II 3G Ex nA T4, Messbereich: 1 / 2,5 / 5 / 10 / 20 m/s (uni- oder bidirektional), Druck: atmosphärisch 700 ... 1300 hPa, Betriebsspannung : 12 ... 24 VDC, Ausgang: 0 / 4...20mA, 0 ... 2V / 5V / 10V

Kontakt:
SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen, Tel.:  +49/7724/899-0 Fax:+49/7724/899101, Email: info@schmidttechnology.de, Homepage: www.schmidttechnology.de

SCHMIDT® Flow-sensor SS 23.400 ATEX3 

SCHMIDT Technology expands the range of products by offering a new thermal flow sensor for the use in explosive environment. Designed for the operation according the ATEX-directives, the sensor falls in the category 3G and can be applied in ATEX-zone 2.

The insertion sensor with a 9 mm stainless steel tube can measure the flow velocity and detect the direction of clean air and gas flow. The microcontroller based electronic unit is integrated in the tube. The precise sensors tip contains a super fast sensor element in an aerodynamically designed and mechanical protected chamber.
The analogue output for the measuring result provides a voltage or current signal. Two switching outputs indicate the flow direction and a limit value.
A serial interface allows on-site programming of the sensor via PC and the adaptation of, response time, threshold and switching polarity to the operation requirements.
Applications: paint-spray lines, gas flow measuring, exhaust monitoring, flow measuring in medical equipments and test plants
Technical Data: device identification II 3G Ex nA T4, measuring range: 1 / 2,5 / 10 / 20 m/s (in both directions), Pressure: atmospheric, 700 ...1300 hPa, power supply: 12 … 24 VDC, Outputs: 0 / 4 ... 20 mA, 0 … 2V / 5V / 10V

Contact:
SCHMIDT Technology GmbH, Feldbergstr. 1, 78112 St. Georgen,Tel.:  +49/7724/899-0 Fax:+49/7724/899101, Email: info@schmidttechnology.de, Homepage: www.schmidttechnology.de