5. All Functions
<MagneW 2W>
Displays all available functions.
Some parameters in the high/low
limit alarm or pulse menus may
not be shown, depending upon the
selected functions.
The open collector menu offers
selection of high/low limit alarm
or pulse output. If high/low limit
alarm is selected, parameters for
the pulse output are not shown.
If the pulse output is selected,
parameters for high/low limit
alarm function are not shown.
The opt. functions, dual range
and error history is not
available on the MagneW 2W.
<MagneW 4W>
Displays all available functions.
Some parameters in the dual range,
high/low limit alarm menus may
not be shown depending on the
model or selected function.
Parameters in the dual range menu
are displayed by selecting an
appropriate ranging setting in the
opt. functions menu.
Parameters for high/low limit alarm
are shown by selecting an
appropriate function for contact
output in the opt. functions menu.
The open collector output and the
empty configuration is not available
on the MagneW 4W.