14. Memo
Displays and writes memo 1 and memo
2.
Tap the memo 1 or memo 2 to modify
its value. Tap the enter key to confirm
the value, and then tap [Send] to
transmit the data to the valve positioner.
If you have not yet tapped [Send], and
want to recall the previous memo, tap
[Read].
Up to 16 characters may be entered for
each memo.
Valid characters are A-Z, 0-9, space,
period, hyphen, and slash. Lowercase a-
z will be capitalized to A-Z.