12. Flow Type
Sets flow characteristics.
Select Linear, Equal Percent, Quick
Open, or User-defined from the combo
box.
Tap [Send] to transmit the changes to
the valve positioner. If you have not
yet tapped [Send], and want to recall
the previous data, tap [Read].
Select user-defined to display the
change user-defined data button. This
option allows setting of 16-point
polygonal line approximation data. The
16 point data is displayed over 2
pages. Tap [P9-16>] or [<P1-8] to
move between pages.
Tap any display field to display the
input screen. Input the desired value
and tap [Enter].
Tap [Send] to transmit the changes to
the valve positioner. If you have not
yet tapped [Send], and want to recall
the previous data, tap [Read].
Tap [Cancel] to return to the previous
screen.
Tap [Graph] to graph and check the
new characteristics.