7. Conformity
Displays the following items.
-- Conformity: Select from linear or
square root (flow).
-- Cutoff: Select a value below which
the flow output is cut off. Output
below this value will behave
according to the dropout setting.
-- Dropout: Select behavior below the
cutoff value. Select either zero or
linear.
-- Flow mode: Select calculation
method of flow output. Select either
default (square root of positive
output) or bi-direction (square root
of both positive and negative
outputs).