16. Display
Sets the display conformity and
display units.
-- Display Conformity: Linear or flow
(square root extraction)
-- Display Unit: % actual press.
(pressure) or eng. unit
(engineering unit)
-- Actual Press.: Displays actual
measured pressure in the
selected unit of measurement.
-- Engineering unit: Displays value
according to user-defined scale
and unit (flow rate, level etc.).
EULO (0%) and EUHI (100%) may
be set up when eng. unit is selected.
EULO: Low limit of the engineering
unit scale, corresponding to 0%
input, is displayed on the indicator.
EUHI: High limit of the engineering
unit scale, corresponding to 100%
input, is displayed on the indicator.